

Press information

To download a 300dpi print quality image, go to [parkfield.co.uk/hammond-usa/industrial-print.jpg](http://www.parkfield.co.uk/hammond-usa/industrial-print.jpg)

To download a Word file of the text, go to [parkfield.co.uk/hammond-usa/industrial.docx](http://www.parkfield.co.uk/hammond-usa/industrial.docx)

To view all Hammond Manufacturing press information, go to [parkfield.co.uk/hammond-usa/](http://www.parkfield.co.uk/hammond-usa/)

**IP66 sealed polycarbonate and ABS enclosures for industrial applications  
Released September 27, 2018**Optimized for use in harsh industrial environments, the [1554 flat lid](https://www.hammfg.com/electronics/small-case/plastic/1554) and [1555 styled lid](https://www.hammfg.com/electronics/small-case/plastic/1555) ranges of ABS and UV stabilized polycarbonate enclosures from Hammond Manufacturing provide IP66 sealing and good mechanical protection. The light grey RAL 7035 enclosures are designed to house printed circuit boards or DIN rail mounted components. IP66 sealing is achieved through a one piece silicone gasket in a tongue and groove seal. 23 sizes from 2.60 x 2.60 x 1.60 inches (66 x 66 x 41 mm) to 9.40 x 6.30 x 4.70 inches  
(239 x 160 x 119 mm) are available with flat and styled self colored, clear and translucent lids. [Flanged lids](https://www.hammfg.com/electronics/small-case/plastic/1555f) for 10 sizes, from 4.70 x 2.60 x 1.65 inches (119 x 66 x 42 mm) to 7.10 x 4.70 x 2.44 inches   
(180 x 119 x 62 mm), provide increased security by preventing access to the interior without removing the enclosure from the surface to which it is attached.

The styled lids include a recess suitable for mounting a membrane keyboard and are also fitted with PCB mounting bosses. Bases are fitted with internal DIN rail mounting tabs in all but two sizes and standoffs for mounting PCBs or optional internal panels are provided in all versions.

To avoid any possible corrosion problems the base inserts and self-captivating lid screws are both stainless steel, located outside the gasket; additional holes in the base, again outside the gasket seal are provided to allow the enclosure to be wall or shelf mounted. An optional foot kit is also available. Optional steel panels suitable for mounting heavy components can be fitted to the integral mounting points in the base; the bases also feature molded slots to enable 1.6mm thick PCBs to be mounted vertically into the enclosure.

\*\*\* Ends: body copy 267 words \*\*\*

**Notes to Editors.**

For further information contact:

Ray Shatzel

Hammond Manufacturing Co. Inc.

475 Cayuga Rd.

Cheektowaga

NY 14225-1309   
Tel: (716) 630-7030

Fax: (716) 630-7042

[rshatzel@hammfg.com](mailto:rshatzel@hammfg.com)

[www.hammondmfg.com](http://www.hammondmfg.com)

Agency contact:

Nigel May

Parkfield Communications Limited

Parkfield House

Damerham

Hants

SP6 3HQ

United Kingdom

tel: + 44 1725 518321

fax: + 44 1725 518378

[nigel.may@parkfield.co.uk](mailto:nigel.may@parkfield.co.uk)

[www.parkfield.co.uk](http://www.parkfield.co.uk)

Hammond is one of the world’s leading manufacturers of small plastic, die-cast and metal enclosures for use in the electronics, electrical and allied industries.