**Press information**

To download a 300dpi print quality image, go to [parkfield.co.uk/bvm/inox-f15c-ult3-print.jpg](http://www.parkfield.co.uk/bvm/inox-f15c-ult3-print.jpg)

To download a Word file of the text, go to [parkfield.co.uk/bvm/inox-f15c-ult3.docx](http://www.parkfield.co.uk/bvm/inox-f15c-ult3.docx)

To view all BVM press information, go to [parkfield.co.uk/bvm/](http://www.parkfield.co.uk/bvm/)

**Waterproof Panel PC for demanding applications**

**Released 21 August 2018**

The new [INOX-F15C-ULT3](http://www.bvm.co.uk/ProductDetail.asp?fdProductId=1303) 15 inch Panel PC from BVM Limited is housed in a monolithic 304 stainless steel enclosure sealed to IP69k, the most demanding environmental protection specification. Designed to be installed in environments such as the food processing industry, where it will be subjected to regular high pressure, high temperature washing, the F15C–ULT3 is suitable for other applications in the industrial, marine and pharmaceutical sectors where a physically rugged self-contained PC is going to be exposed to high levels of dust, water and temperature. The unit is third-party IP69K tested with an 80°C 80 -100 bar water jet at 100 – 150mm distance at angles from 0 to 90°.

The fanless PC is based on the Intel Skylake ULT chipset running 6th generation Intel Core i5 and Celeron ULT processors with up to 32GB of DRAM. The integral 10 point touchscreen is fitted with an anti-UV protective coating. Two 10G LAN ports, two COM serial ports and two USB2.0 ports are provided as standard; the interface for all I/O is via M12 sealed connectors. Also externally accessible is a 2.5 inch SATAIII bay for mass storage. Expansion capability is a full-size PCIe Mini card slot, a full-size/half-size (PCIe x1 and USB 2.0 signals slot and a M.2 B-key slot. 12VDC @ 5A power-in is from an external 90 – 264 VAC PSU via a sealed connector.

\*\*\* Ends: body copy 225 words \*\*\*

**Notes to Editors.**

Technical and sales contact for publication:

David Harding

BVM Limited

Lakeside House

Waltham Business Park

Brickyard Road

Swanmore

SO32 2SA

t: + 44 (0)1489 780144

f: + 44 (0)1489 783589

[sales@bvmltd.co.uk](mailto:sales@bvmltd.co.uk)

[bvm.co.uk/](http://www.bvm.co.uk/)

Editorial contact:

Rod Clarke

t: + 44 (0)1489 780144

[rod\_c@bvmltd.co.uk](mailto:rod_c@bvmltd.co.uk)

Agency contact:

Nigel May

Parkfield Communications Ltd

Parkfield House

Damerham

Hants

SP6 3HQ

t: + 44 (0)1725 518321

f: + 44 (0)1725 518378

[nigel.may@parkfield.co.uk](mailto:nigel.may@parkfield.co.uk)

[parkfield.co.uk](http://www.parkfield.co.uk)